| genesis menu simulator |
| cancel | counter clock | push down | clockwise |  |
| This page changes H phase with regard to an incoming video reference, and controls color bar type and output.
| Note To synchronize the shutters of multiple cameras, take Genlock out of 1 camera and loop through the others. Do not put a Genlock in to the first camera.
| The H PHASE control is for technician use.
| COLOR BAR
| ON will put color bars on the output of the camera Panavision recommends using HD-SMPTE color bars are because it permits setting the black level on the monitor accurately
| COLOR BAR ON and OFF is more easily accessed by using page U1 or the LCD Menu Panel on the camera body
| While color bars are useful for setting monitors and checking video levels, Panavision recommends shooting grey charts for post-production calibration.
| help | top menu | comments/corrections? |