| genesis menu simulator |
| cancel | counter clock | push down | clockwise |  |
| Display of the voltage levels that will set off battery warnings, and those below which the camera will shut down.
| This page is identical to page 7 of the Operation menu
| Values in parentheses cannot be changed by user
| The top half concerns the 24 Volt input
| TYPE
| AC ADP means AC Adapter
| BEFORE END is the voltage at which battery warning will appear
| END is the voltage at which camera will shut down
| The bottom half concerns the 12 Volt input
| TYPE
| AC ADP means AC Adapter
| BEFORE END is the voltage at which battery warning will appear
| END is the voltage at which camera will shut down
| help | top menu | comments/corrections? |