| genesis menu simulator |
| cancel | counter clock | push down | clockwise |  |
| This page is used to set frame lines
| CENTER TYPE selects 1 of 4 types of center cross hairs.
| SAFETY SIZE selects the percentage area of the 16by9 SAFETY frame
| Every frame line can be displayed in each of 3 separate outputs: VF1 and VF2 (the two viewfinder multipin plugs on camera front) and MONI (the HDSDI BNC plug on side of camera). Usually VF1 is used for the viewfinder, and MONI goes to the on-board monitor, and then onwards to other on-set monitors.
| Each of the following frame lines can be individually turned ON and OFF for each of the 3 outputs:
| MARKER - turns all frame lines on or off CENTER - is the center cross hair selected above in CENTER TYPE SAFETY - is a 16by9 safety determined by the SAFETY SIZE above EFFECT - is the 16by9 "full aperture" or "effective" pixel area CURSOR - is the user-definable frame you will use to sketch out 1.85, 2.40 and any other format that is not 1.78
| Note that the when MARKER is ON in this page, all the frame lines can then be toggled ON or OFF by means of a switch on the SONY Viewfinder. To toggle: repeatedly click top switch leftwards toward ASPECT.
| help | top menu | comments/corrections? |