| genesis menu simulator |
| cancel | counter clock | push down | clockwise |  |
| This page allows users to change different gain parameters for Red, Green, Blue and Master.
| As depicted here, Panavision recommends leaving all VIDEO LEVELs at 0.
| FILM TYPE changes the color response of the camera
| TUNGSTEN is used with 3200 Kelvin lighting DAYLIGHT is used with daylight or 5600 Kelvin lighting, although some cinematographers will prefer to use an 85 filter in front of or behind the lens.
| You can also change Film Type on page U1, or on the camera LCD panel
| As pictured here, Panavision recommends leaving FLARE OFF
| help | top menu | comments/corrections? |