| genesis menu simulator |
| cancel | counter clock | push down | clockwise |  |
| A varied page with controls for fan, date, image inversion, menu language, LCD contrast and characters out.
| FAN MODE controls the modes and noise of the camera built-in fan
| AUTO1 is the Panavision recommended mode. VTR fans are off during recording, quiet low-speed fans in the camera stay on. AUTO2 MIN - minimum fan, Panavision does not recommend this mode MAX - maximum fan, use when camera is very hot.
| The MAX FAN MODE is often attributed to an ASSIGNABLE SWITCH, see page 8 of the Operation Menu.
| MENU RESUME
| ALL is the Panavision recommended mode. TOP OPE OFF
| DATE TYPE for selection of the format of the DATE on page M5
| IMAGE INVERT will invert the image output
| LANGUAGE determines terminology for the following menu items:
| FILM | VIDEO |  |
| STOPS | DBS |  |
| TUNGSTEN | 3200K |  |
| DAYLIGHT | 5600K |  |
| SHUTTER ANGLE | FRACTION OF SECOND |
| LCD CONTRAST adjust contrast on LCD panel on camera body
| MONO CHAR if you know what this does please email benjaminb.mail@free.fr
| help | top menu | comments/corrections? |