| genesis menu simulator |
| cancel | counter clock | push down | clockwise |  |
| The SHUTTER and ECS menu items can be more easily accesed on page U1 or on the LCD menu panel on the camera body.
| SHUTTER controls the electronic shutter and determines the effective exposure time for each frame, just as in film.
| SHUTTER ON enables the range of shutter angles The available options are ??? ECS is selected for all other shutter speeds, the angle is determined below
| SHUTTER OFF is the equivalent of a 360 degree shutter. It yields 1 more stop of exposure than a traditional 180 degree It yields an effective exposure time of 1/12 sec at 24 fps It increases motion blur, and reduces apparent strobing
| ECS ANGLE is user-defined shutter angles. Pictured here is the European and Australian standard setting of 172.8 degrees.
| ECS is also used to eliminate horizontal bars when shooting CRT monitors. ECS stands for Extended Clear Scan, an old video term
| help | top menu | comments/corrections? |