| genesis menu simulator |
| cancel | counter clock | push down | clockwise |  |
| This page allows you to transfer reference settings to or from either the in-camera memory or an external Memory Stick
| The following parameters are stored in the Reference File: ?????????
| To restore the Panavision Default scene settings
| Click on STANDARD
| To store your current settings as the standard
| Click on STORE FILE
| To use a Memory Stick to retrieve or store user defined settings:
| Insert Memory Stick FILE ID will display user-defined name or 14 blank box characters CAM CODE will display camera type DATE will be displayed
| To retrieve previously recorded settings
| 5a. Click READ (MS->CAM) to retrieve settings from the Memory Stick
| To store your current settings
| 5b1. You have the option to change the FILE ID by selecting alphanumeric characters
| 5b2. Click WRITE (CAM->MS) to record your settings on to the Memory Stick
| help | top menu | comments/corrections? |