| genesis menu simulator |
| cancel | counter clock | push down | clockwise |  |
| This page is only active when variable frame rates are selected on page M6
| The FPS setting can be more easily accessed on page U1 or on the LCD Menu Panel on the camera body.
| VIDEO-LVL determines whether the camera will compensate for the change in video level due to a different exposure time than the chosen format (24P in this example). For example a 12 FPS setting entails twice the exposure of 24 P.
| ACCUM - short for accumulate: no compensation will be done, resulting in overexposure when shooting at slow speeds. CONST (GAIN) - short for constant: the gain will vary to compensate for exposure change CONST (SHUT) - the shutter will vary to compensate for exposure change
| VF SCAN determines whether the camera will compensate for the change in the image refresh rate
| NORMAL - the image is refreshed at the format rate (24P in this example) ACCUM - the image is refreshed at the FPS rate, resulting in a flickering image at low FPS speeds.
| help | top menu | comments/corrections? |